{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"This example uses the DMM6500 with the 2001-TCSCAN card  to perform",null,null,null,null,null,"У цьому прикладі використовується DMM6500 з картою 2001-TCSCAN для виконання"]
[null,null,null,"temperature scanning using the CJC sensor (channel 1) of the scan card to",null,null,null,null,null,"сканування температури за допомогою датчика CJC (канал 1) скануючої карти для"]
[null,null,null,"provide corrected thermocouple-based measurements on channels 2 - 4.",null,null,null,null,null,"забезпечити коректні вимірювання на основі термопар на каналах 2 - 4."]
[null,null,null,"All channels will be sampled once per minute for 2 hours. ",null,null,null,null,null,"Всі канали будуть вибірку робити раз на хвилину протягом 2 годин. "]
[]
[null,null,null,null,null,null,null,null,null,"KEITHLEY INSTRUMENTS,MODEL DAQ6510,04623890,1.7.12b"]
[]
[]
[null,null,null,null,"CH1","CH2","CH3","CH4"]